756

| DASHBOARD WIRING
DG

#### 756
AIR BAG/PRETENSIONER COMPUTER
EBASE/ABLAV EBASE/SABLAT CA,CAREG/SSESP CA,CAREG/ASRESP

21 | 0.35 | 60DS | PASSENGER AIR BAG INHIBITOR KEY SIGNAL
22 | 0.35 | 60DT | - PASSENGER AIR BAG INHIBITOR KEY
1 | 0.5 | 60L | LEVEL 2 PASSENGER'S FRONT AIR BAG + CONTROL
2 | 0.5 | 60H | PASSENGER EUROBAG + SIGNAL
3 | 0.35 | 60AM | LEVEL 1 DRIVER'S FRONT AIR BAG + CONTROL
4 | 0.35 | 60AP | LEVEL 2 DRIVER'S FRONT AIR BAG + CONTROL
7 | 0.35 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION
10 | 0.35 | 133C | INSTRUMENT PANEL CAN L SIGNAL > COMPUTER
11 | 0.35 | 133B | INSTRUMENT PANEL CAN H SIGNAL > COMPUTER
12 | 0.5 | 60M | LEVEL 2 PASSENGER'S FRONT AIR BAG - CONTROL
13 | 0.5 | 60K | PASSENGER'S FRONT AIR BAG LEVEL 1 - CONTROL
14 | 0.35 | 60AN | LEVEL 1 DRIVER'S FRONT AIR BAG - CONTROL
15 | 0.35 | 60AQ | LEVEL 2 DRIVER'S FRONT AIR BAG - CONTROL
18 | 0.5 | NAP | TUNNEL ELECTRONIC EARTH