R301

| CONNECTION
ANY TYPE

#### R301
DASHBOARD/COURTESY LIGHT CONNECTION
DG EBASE/ABLAV DG EBASE/SABLAT DG CA,CAREG/SSESP

11 | 0.35 | 107G | HANDS FREE TELEPHONE MICROPHONE +
12 | 0.35 | 107H | HANDS FREE TELEPHONE MICROPHONE -
13 | 0.35 | BPT | PROTECTED + BATTERY FEED TIMER
14 | 0.35 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
15 | 0.35 | 13E | INTERIOR LIGHTS - CONTROL > TIMER
19 | 0.35 | 47F | VEHICLE SPEED SIGNAL
20 | 0.35 | 21K | ANTI-PINCH SUNROOF/ELECTRIC WINDOW SERIAL LINE SIGNAL
21 | 1.0 | BP93 | + BATTERY PROTECTED SUNROOF
22 | 1.0 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
1 | 0.35 | AP1A | ROOF FUSE PROTECTED + AFTER IGNITION
2 | 0.35 | 14S | RAIN SENSOR SERIAL LINE SIGNAL
3 | 0.5 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
7 | 0.35 | 38GZ | INTERIOR TEMPERATURE SENSOR SIGNAL
8 | 0.35 | 38JN | SUN TEMPERATURE HUMIDITY SENSOR ZERO VOLTS