1303

| RADIO/MULTIMEDIA DISPLAY INTERMEDIATE WIRING
DG

#### 1303
VIDEO SCREEN RETRACTION UNIT
RAD03/NINAV3

1 | 0.5 | BCP3 | PROTECTED + BATTERY FEED CIRCUIT BREAKER INTERIOR LIGHT FUSE
7 | 0.5 | MAN | DASHBOARD RIGHT-HAND CROSS MEMBER ELECTRICAL EARTH
9 | 0.35 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
13 | 0.35 | 46BC | NAVIGATION CAN L SIGNAL
14 | 0.35 | 46BB | NAVIGATION CAN H SIGNAL 1
15 | 0.35 | 34GA | MULTIMEDIA 1 CAN L SIGNAL
16 | 0.35 | 34DZ | MULTIMEDIA 1 CAN H SIGNAL
17 | 0.35 | 34GD | COMMUNICATION START/STOP SIGNAL 1
18 | 0.35 | 46AD | NAVIGATION ON/OFF CONTROL