R34

| CONNECTION
ANY TYPE

#### R34
ENGINE/DASHBOARD CONNECTION
F4R770,F4R771 BVA4/TLMEXI F4R770,F4R771 BVA4/SSTLMEXI K4M760

1 | 0.75 | HK | DIAGNOSTIC SIGNAL K
2 | 0.75 | 5DU | GEAR LEVER LOCKING - CONTROL
3 | 0.75 | 5H | N+1 PUSH BUTTON CONTROL
4 | 0.75 | 5FM | LOWER CONTACT MULTIFUNCTION PUSH BUTTON CONTROL
5 | 0.75 | 5A | BRAKE PEDAL SWITCH + SIGNAL
6 | 0.75 | 5CQ | AUTOMATIC GEARBOX DISPLAY SIGNAL