R369

| CONNECTION
ANY TYPE

#### R369
DASH BOARD / MULTIMEDIA CONNECTION
DG EBASE/ABLAV DG CA,CAREG/SSESP DG CA,CAREG/ASRESP DD

3 | 1.0 | 34E | RIGHT HAND FRONT LOUDSPEAKER + SIGNAL
4 | 0.5 | 34F | RIGHT HAND FRONT LOUDSPEAKER - SIGNAL
4 | 1.0 | 34F | RIGHT HAND FRONT LOUDSPEAKER - SIGNAL
5 | 0.5 | 34G | LEFT HAND FRONT LOUDSPEAKER + SIGNAL
5 | 1.0 | 34G | LEFT HAND FRONT LOUDSPEAKER + SIGNAL
6 | 0.5 | 34H | LEFT HAND FRONT LOUDSPEAKER - SIGNAL
6 | 1.0 | 34H | LEFT HAND FRONT LOUDSPEAKER - SIGNAL
7 | 1.0 | 34A | LEFT HAND REAR LOUDSPEAKER + SIGNAL
8 | 1.0 | 34B | LEFT HAND REAR LOUDSPEAKER - SIGNAL
1 | 1.0 | 34D | RIGHT HAND REAR LOUDSPEAKER + SIGNAL
2 | 1.0 | 34C | RIGHT HAND REAR LOUDSPEAKER - SIGNAL
3 | 0.5 | 34E | RIGHT HAND FRONT LOUDSPEAKER + SIGNAL