1337

| DASHBOARD WIRING
DG

#### 1337
SWITCHING PROTECTION UNIT
CA,CAREG/SSESP CA,CAREG/ASRESP

1 | 1.0 | 14L | WINDSCREEN WIPER TIMER HIGH SPEED + CONTROL
2 | 0.5 | 14K | WINDSCREEN WIPER TIMER LOW SPEED + CONTROL
3 | 1.4 | NAM | UPPER LEFT-HAND CROSS MEMBER ELECTRONIC EARTH
4 | 1.0 | CPD | PROTECTED RIGHT HAND DIPPED BEAM HEADLIGHT +
5 | 1.4 | 3N | FUEL PUMP +
6 | 1.0 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
7 | 1.0 | LPD | PROTECTED RIGHT HAND SIDE LIGHT +
8 | 1.4 | APCB | + AFTER IGNITION PROTECTED / COLUMN LOCK FUSE CONTACT CLOSED AT REST
9 | 0.5 | H66P | REVERSING LIGHTS + CONTROL
10 | 0.35 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION
10 | 0.35 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION
11 | 2.0 | AP43 | PROTECED + AFTER IGNITION FUSE