971

| ENGINE WIRING
F4R770,F4R771

#### 971
"DP0" AUTOMATIC GEARBOX MODULE
BVA4/TLMEXI BVA4/SSTLMEXI

A1 | 0.5 | H66P | REVERSING LIGHTS + CONTROL
B1 | 0.75 | 5BB | SEQUENCE SOLENOID VALVE 6 -
C1 | 0.75 | 5U | LINE PRESSURE SENSOR +
D1 | 0.75 | 5DA | GEARBOX INPUT SPEED SENSOR + SIGNAL
A2 | 0.5 | AP11 | PROTECTED + AFTER IGNITION REVERSING LIGHTS FUSE
B2 | 0.75 | 5DM | MODULATING SOLENOID VALVE 4
C2 | 0.75 | 5W | LINE PRESSURE SENSOR + SIGNAL
D2 | 0.75 | 5DB | GEARBOX INPUT SPEED SENSOR - SIGNAL
B3 | 1.0 | 5AU | SEQUENCE SOLENOID VALVE +
C3 | 0.75 | 5V | LINE PRESSURE SENSOR -
B4 | 0.75 | 5BC | PRESSURE SOLENOID VALVE 1 -
B5 | 0.75 | 5DL | MODULATING SOLENOID VALVE 3
B6 | 1.0 | 5BX | BRIDGING MODULATING SOLENOID VALVE
A7 | 0.75 | 5DK | MULTIFUNCTION SWITCH - > AUTOMATIC TRANSMISSION COMPUTER
B7 | 0.75 | 5AY | SEQUENCE SOLENOID VALVE 4 -
B8 | 0.75 | 5AW | SEQUENCE SOLENOID VALVE 2 -
B9 | 1.0 | 5AZ | SEQUENCE SOLENOID VALVE 5 -
A10 | 0.75 | 5DG | MULTIFUNCTION SWITCH SIGNAL 2
B10 | 0.75 | 5AX | SEQUENCE SOLENOID VALVE 3 -
A11 | 0.75 | 5DH | MULTIFUNCTION SWITCH SIGNAL 3
B11 | 0.75 | 5AV | SEQUENCE SOLENOID VALVE 1 -
A12 | 0.75 | 5DJ | MULTIFUNCTION SWITCH SIGNAL 4
B12 | 1.0 | 5BA | MODULATING SOLENOID VALVE +