239

| DRIVER'S DOOR WIRING
X84

#### 239
DRIVER'S ELECTRIC REAR-VIEW MIRROR
B84,S84/DG/EPACK B84,S84/DG/EPACKP

1 | 0.35 | 15RP | PROTECTED HEATED REAR VIEW MIRROR + CONTROL
2 | 0.35 | 40C | DRIVER'S REAR VIEW MIRROR UP/DOWN CONTROL
3 | 0.35 | 40E | REAR VIEW MIRROR MOTOR COMMON
3 | 0.35 | 40E | REAR VIEW MIRROR MOTOR COMMON
4 | 0.35 | 40A | DRIVER'S REAR VIEW MIRROR RIGHT>LEFT CONTROL
5 | 0.35 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
7 | 0.35 | 40X | REAR-VIEW MIRROR FOLD OUT CONTROL
9 | 0.35 | 40W | REAR-VIEW MIRROR FOLD IN CONTROL