1076

| ENGINE WIRING
K4J730,K4M764

#### 1076
MOTORISED THROTTLE BODY
K4J730/CHAUFO K4J730/CA,CAREG K4M764/EQGPL

1 | 0.5 | 3MO | MOTORISED THROTTLE POTENTIOMETER SENSOR -
2 | 0.5 | 3MP | MOTORISED THROTTLE POTENTIOMETER 1 SIGNAL
3 | 1.4 | 3AJC | THROTTLE MOTOR - CONTROL
4 | 1.4 | 3AJB | THROTTLE MOTOR + CONTROL
5 | 0.5 | 3MN | MOTORISED THROTTLE POTENTIOMETER + 5 VOLTS
6 | 0.5 | 3MQ | MOTORISED THROTTLE POTENTIOMETER 2 SIGNAL