261

| RADIO/MULTIMEDIA DISPLAY INTERMEDIATE WIRING
DG

#### 261
RADIO
PRETEL/RAD02,RAD03/SSNAV RAD05,RAD06/SSNAV RAD03/NINAV3 RAD06

1 | 0.35 | 47F | VEHICLE SPEED SIGNAL
3 | 0.35 | 107D | TELEPHONE RADIO CUT-OFF SIGNAL
4 | 1.0 | BCP3 | PROTECTED + BATTERY FEED CIRCUIT BREAKER INTERIOR LIGHT FUSE
5 | 0.35 | 34AM | WAVE SEPARATOR AERIAL AMPLIFIER +
6 | 0.35 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
7 | 1.0 | SP2 | PROTECTED + ACCESSORIES > RADIO
8 | 3.0 | MAO | DASHBOARD CROSS MEMBER RADIO EARTH