R4

| CONNECTION
ANY TYPE

#### R4
DASHBOARD/PASSENGER'S DOOR CONNECTION
DG EBASE/ABLAV DG EBASE/SABLAT

1 | 1.4 | 22D | FRONT ELECTRIC WINDOW CONTROL 2
2 | 0.5 | 20BK | PASSENGER DOORS / REAR DOORS LOCKING MOTOR CONTROL
3 | 0.5 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL
4 | 0.22 | 87G | PASSENGER'S 1st POSITION SWITCH - SIGNAL
6 | 1.0 | 34E | RIGHT HAND FRONT LOUDSPEAKER + SIGNAL
7 | 1.0 | 34F | RIGHT HAND FRONT LOUDSPEAKER - SIGNAL
8 | 0.5 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
11 | 2.5 | MAN | DASHBOARD RIGHT-HAND CROSS MEMBER ELECTRICAL EARTH
18 | 0.35 | 47C | EXTERNAL TEMPERATURE SENSOR + SIGNAL
19 | 0.35 | 47D | EXTERNAL TEMPERATURE SENSOR ZERO VOLTS SIGNAL
20 | 1.4 | 22C | FRONT ELECTRIC WINDOW CONTROL 1