R13

| CONNECTION
ANY TYPE

#### R13
LEFT REAR/LEFT-HAND REAR DOOR CONNECTION
B84,S84 EPACKP

3 | 0.35 | 23C | ELECTRIC WINDOW UP CONTROL > LEFT HAND REAR QUARTER LIGHT CLOSE
3 | 0.5 | 23C | ELECTRIC WINDOW UP CONTROL > LEFT HAND REAR QUARTER LIGHT CLOSE
4 | 0.35 | 23D | ELECTRIC WINDOW DOWN CONTROL > LEFT HAND REAR QUARTER LIGHT OPEN
4 | 0.5 | 23D | ELECTRIC WINDOW DOWN CONTROL > LEFT HAND REAR QUARTER LIGHT OPEN
5 | 0.5 | 21K | ANTI-PINCH SUNROOF/ELECTRIC WINDOW SERIAL LINE SIGNAL
6 | 0.35 | 23K | LEFT HAND REAR ELECTRIC WINDOW CONTROL 2
7 | 0.35 | 23J | LEFT HAND REAR ELECTRIC WINDOW CONTROL 1
8 | 0.35 | 20AL | REAR INTERIOR LOCKING CONTROL
9 | 0.5 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
10 | 0.35 | 26AP | KEYLESS VEHICLE LOCKING SIGNAL / DRIVER SIDE DOORS SWITCH
11 | 0.5 | 26P | DOOR HANDLE INFRARED SENSOR +
12 | 0.5 | 26S | DRIVER'S SIDE REAR HANDLE INFRARED SENSOR SIGNAL
13 | 0.35 | BPT2 | + BATTERY PROTECTED TIMED LIGHTING
14 | 0.35 | 13AC | FOOTWELL LIGHTING TIMER + CONTROL
15 | 0.35 | 26AG | KEYLESS VEHICLE DRIVER'S SIDE REAR DOOR EXTERNAL AERIAL A SIGNAL
16 | 0.35 | 26AH | KEYLESS VEHICLE DRIVER'S SIDE REAR DOOR EXTERNAL AERIAL B SIGNAL
21 | 1.0 | 34A | LEFT HAND REAR LOUDSPEAKER + SIGNAL
22 | 1.0 | 34B | LEFT HAND REAR LOUDSPEAKER - SIGNAL
24 | 2.0 | BP87 | REAR ELECTRIC WINDOWS FUSE PROTECTED + BATTERY FEED
25 | 2.5 | MZ | REAR END PANEL ELECTRICAL EARTH
26 | 0.5 | 20BG | REAR DOORS DEADLOCKING STATUS SIGNAL
27 | 0.5 | 20W | REAR DEADLOCKING MOTOR CONTROL
28 | 0.5 | MZ | REAR END PANEL ELECTRICAL EARTH
29 | 0.5 | 87A | LEFT HAND REAR 1st POSITION SWITCH - SIGNAL
30 | 0.5 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL
31 | 0.5 | 20BK | PASSENGER DOORS / REAR DOORS LOCKING MOTOR CONTROL