645

| DASHBOARD WIRING
DG

#### 645
PASSENGER COMPARTMENT COMPUTER
EBASE/ABLAV EBASE/SABLAT CA,CAREG/SSESP CA,CAREG/ASRESP

1 | 0.35 | 13E | INTERIOR LIGHTS - CONTROL > TIMER
1 | 0.35 | 13E | INTERIOR LIGHTS - CONTROL > TIMER
2 | 2.0 | NAM | UPPER LEFT-HAND CROSS MEMBER ELECTRONIC EARTH
3 | 0.75 | BPT | PROTECTED + BATTERY FEED TIMER
4 | 1.0 | 64C | LEFT HAND TURN SIGNAL LIGHTS CONTROL
5 | 1.0 | 64D | RIGHT HAND TURN SIGNAL LIGHTS CONTROL
6 | 0.5 | 9P | PROTECTED REAR FOG LIGHTS + CONTROL
7 | 0.5 | 20S | TAILGATE MOTOR OPENING AUTHORISED FEED
8 | 0.5 | 20AG | REAR SCREEN MOTOR OPENING AUTHORISED FEED
9 | 0.35 | BPT2 | + BATTERY PROTECTED TIMED LIGHTING
10 | 0.35 | 13AC | FOOTWELL LIGHTING TIMER + CONTROL