203

| DRIVER'S DOOR WIRING
X84

#### 203
DRIVER'S WINDOW MOTOR
B84/LVAVEI/DG B84,S84/DG/EPACK B84,S84/DG/EPACKP

1 | 0.5 | 21E | ONE-TOUCH ELECTRIC WINDOW NORMAL DOWN - CONTROL
2 | 0.5 | 21C | ONE-TOUCH ELECTRIC WINDOW NORMAL UP - CONTROL
3 | 2.0 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
4 | 1.4 | BP55 | DRIVER'S ONE-TOUCH ELECTRIC WINDOW FUSE PROTECTED + BATTERY FEED
6 | 0.5 | 21K | ANTI-PINCH SUNROOF/ELECTRIC WINDOW SERIAL LINE SIGNAL