1511

| DRIVER'S DOOR WIRING
X84

#### 1511
DRIVER'S REAR TWIN ELECTRIC WINDOWS CONTROL
B84,S84/DG/EPACK B84,S84/DG/EPACKP DD/CPE

1 | 0.35 | 23H | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 2
2 | 0.35 | 23A | ELECTRIC WINDOW CONTROL > RIGHT-HAND REAR QUARTER LIGHT CLOSE
3 | 0.5 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
4 | 0.35 | 23C | ELECTRIC WINDOW UP CONTROL > LEFT HAND REAR QUARTER LIGHT CLOSE
5 | 0.35 | 23J | LEFT HAND REAR ELECTRIC WINDOW CONTROL 1