247

| DASHBOARD WIRING
DG

#### 247
INSTRUMENT PANEL
EBASE/ABLAV EBASE/SABLAT CA,CAREG/SSESP CA,CAREG/ASRESP

17 | 0.35 | 79F | HEATED SEAT WARNING LIGHT CONTROL
20 | 0.35 | 27A | HANDBRAKE WARNING LIGHT - CONTROL
21 | 0.5 | 30A | BRAKE FLUID LEVEL WARNING LIGHT - CONTROL
25 | 0.35 | 19E | MAIN BEAM HEADLIGHTS - CONTROL > DIMMER
27 | 0.22 | 41A | FUEL LEVEL SENDER + SIGNAL
29 | 0.35 | 80T | ENGINE IMMOBILISER WARNING LIGHT - CONTROL
30 | 0.5 | BCP3 | PROTECTED + BATTERY FEED CIRCUIT BREAKER INTERIOR LIGHT FUSE