1375

| FRONT PASSENGER DOOR WIRING
X84

#### 1375
PASSENGER FRONT DOOR HANDS-FREE CARD DETECTION AERIAL
B84,S84/DD/CPE

1 | 0.35 | 26AC | KEYLESS VEHICLE FRONT PASSENGER DOOR EXTERNAL AERIAL A SIGNAL
2 | 0.35 | 26AD | KEYLESS VEHICLE FRONT RIGHT DOOR EXTERNAL AERIAL SIGNAL 2
3 | 0.35 | 26AQ | KEYLESS VEHICLE LOCKING SIGNAL / PASSENGER SIDE DOORS SWITCH
4 | 0.35 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH