1337

| DASHBOARD WIRING
DD

#### 1337
SWITCHING PROTECTION UNIT
ANY TYPE

1 | 0.35 | AP15 | PROTECTED + AFTER IGNITION ENGINE FUNCTIONS FUSE
3 | 0.5 | SP2 | PROTECTED + ACCESSORIES > RADIO
4 | 0.22 | 32B | OIL LEVEL SENSOR SIGNAL 1
5 | 0.22 | 32A | OIL LEVEL SENSOR SIGNAL 2
6 | 0.35 | 14M | WINDSCREEN WIPER PARK POSITION CONTROL > COMPUTER
7 | 0.5 | 4DN | ANTI-LOCK BRAKING SYSTEM LOWER CAN SIGNAL
8 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL
9 | 0.35 | 3SN | MOTOR 2 CAN L SIGNAL
10 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL
11 | 0.5 | 4DM | ANTI-LOCK BRAKING SYSTEM UPPER CAN SIGNAL
12 | 0.35 | 3SM | MOTOR 2 CAN H SIGNAL