784

| DASHBOARD WIRING
DG

#### 784
COMMAND RELAY BLOCK 2
EBASE/ABLAV CA,CAREG/SSESP CA,CAREG/ASRESP

A1 | 0.5 | SP2 | PROTECTED + ACCESSORIES > RADIO
B1 | 0.5 | SP2 | PROTECTED + ACCESSORIES > RADIO
A2 | 0.35 | 39G | HEADLIGHT WASHERS RELAY 1 + CONTROL
B2 | 0.35 | 39H | HEADLIGHT WASHERS RELAY 2 + CONTROL
A3 | 1.4 | 39A | HEADLIGHT WASHER PUMP + CONTROL
B3 | 1.4 | 39C | HEADLIGHT WASHER PUMP MOTOR CONTROL
A4 | 1.4 | MAS | FRONT LEFT-HAND SIDE MEMBER ELECTRONIC EARTH
B4 | 1.4 | MAS | FRONT LEFT-HAND SIDE MEMBER ELECTRONIC EARTH
A5 | 1.4 | BP32 | PROTECTED + BATTERY FEED HORN FUSE
B5 | 1.4 | BP32 | PROTECTED + BATTERY FEED HORN FUSE