653

| RADIO/MULTIMEDIA DISPLAY INTERMEDIATE WIRING
DG

#### 653
CLOCK/EXTERNAL TEMPERATURE/CARPHONE DISPLAY ASSEMBLY
PRETEL/RAD02,RAD03/SSNAV RAD05,RAD06/SSNAV

4 | 0.35 | 47Z | EXTERNAL TEMPERATURE / DISPLAY SIGNAL
5 | 0.5 | MAN | DASHBOARD RIGHT-HAND CROSS MEMBER ELECTRICAL EARTH
6 | 0.35 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
7 | 0.35 | 19E | MAIN BEAM HEADLIGHTS - CONTROL > DIMMER
8 | 0.5 | SP2 | PROTECTED + ACCESSORIES > RADIO
9 | 0.5 | BCP3 | PROTECTED + BATTERY FEED CIRCUIT BREAKER INTERIOR LIGHT FUSE
11 | 0.35 | 34V | I2C RADIO (TYPE OF RADIO) EARTH SCREENING SIGNAL
12 | 0.35 | 34Z | RADIO OPERATING SIGNAL
13 | 0.35 | 34S | 12C RADIO (TYPE OF RADIO) DATA BUS (INTERFACE) SIGNAL
14 | 0.35 | 34T | I2C RADIO (TYPE OF RADIO) CLOCK SIGNAL
15 | 0.35 | 34U | I2C RADIO (TYPE OF RADIO) MARKING SIGNAL