645

| DASHBOARD WIRING
DD

#### 645
PASSENGER COMPARTMENT COMPUTER
ANY TYPE

3 | 0.5 | 26P | DOOR HANDLE INFRARED SENSOR +
4 | 0.35 | 26AR | KEYLESS VEHICLE LEVEL 2 LOCKING SIGNAL / BOOT LID SWITCH
5 | 0.5 | 20G | TAILGATE MOTOR OPEN CONTROL
6 | 0.35 | 26AQ | KEYLESS VEHICLE LOCKING SIGNAL / PASSENGER SIDE DOORS SWITCH
13 | 0.35 | 39G | HEADLIGHT WASHERS RELAY 1 + CONTROL
14 | 0.35 | 39H | HEADLIGHT WASHERS RELAY 2 + CONTROL
15 | 0.35 | 20AH | OPENING REAR SCREEN STATUS SIGNAL
16 | 0.35 | 20J | REAR SCREEN MOTOR OPEN