R325

| CONNECTION
ANY TYPE

#### R325
PASSENGER COMPARTMENT/AFTER-MARKET ALARM WIRING CONNECTION
DG EBASE/ABLAV DG EBASE/SABLAT DG CA,CAREG/SSESP

1 | 0.5 | BCP3 | PROTECTED + BATTERY FEED CIRCUIT BREAKER INTERIOR LIGHT FUSE
2 | 0.5 | SP2 | PROTECTED + ACCESSORIES > RADIO
3 | 0.35 | 64Q | FLASHER UNIT TIMER - CONTROL
3 | 0.35 | 64Q | FLASHER UNIT TIMER - CONTROL
4 | 0.35 | 80T | ENGINE IMMOBILISER WARNING LIGHT - CONTROL
4 | 0.35 | 80T | ENGINE IMMOBILISER WARNING LIGHT - CONTROL