R243

| CONNECTION
ANY TYPE

#### R243
RIGHT-HAND REAR DOOR/REAR LEFT-HAND WIRING CONNECTION
X84 B84,S84/DG/SPRGAZ/EPACK X84 B84,S84/DG/EQGPL/EPACK

3 | 0.35 | 23A | ELECTRIC WINDOW CONTROL > RIGHT-HAND REAR QUARTER LIGHT CLOSE
4 | 0.35 | 23B | ELECTRIC WINDOW DOWN CONTROL > RIGHT HAND REAR QUARTER LIGHT OPEN
5 | 0.35 | 21K | ANTI-PINCH SUNROOF/ELECTRIC WINDOW SERIAL LINE SIGNAL
6 | 0.35 | 23G | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 1
7 | 0.35 | 23H | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 2
8 | 0.35 | 20AL | REAR INTERIOR LOCKING CONTROL
9 | 0.35 | LPG | PROTECTED LEFT HAND SIDE LIGHT +
13 | 0.35 | BPT2 | + BATTERY PROTECTED TIMED LIGHTING
14 | 0.35 | 13AC | FOOTWELL LIGHTING TIMER + CONTROL
21 | 1.0 | 34D | RIGHT HAND REAR LOUDSPEAKER + SIGNAL
22 | 1.0 | 34C | RIGHT HAND REAR LOUDSPEAKER - SIGNAL
24 | 2.0 | BP87 | REAR ELECTRIC WINDOWS FUSE PROTECTED + BATTERY FEED
25 | 2.5 | MAQ | REAR RIGHT-HAND END PANEL ELECTRICAL EARTH
26 | 0.5 | 20BK | PASSENGER DOORS / REAR DOORS LOCKING MOTOR CONTROL
27 | 0.5 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL
28 | 0.35 | 87B | RIGHT HAND REAR 1st POSITION SWITCH - SIGNAL
29 | 0.35 | MAQ | REAR RIGHT-HAND END PANEL ELECTRICAL EARTH
30 | 0.5 | 20W | REAR DEADLOCKING MOTOR CONTROL
31 | 0.35 | 20BG | REAR DOORS DEADLOCKING STATUS SIGNAL
10 | 0.35 | 26AQ | KEYLESS VEHICLE LOCKING SIGNAL / PASSENGER SIDE DOORS SWITCH
11 | 0.5 | 26P | DOOR HANDLE INFRARED SENSOR +
12 | 0.35 | 26Q | PASSENGER SIDE DOOR HANDLE INFRARED SENSOR SIGNAL
15 | 0.35 | 26AK | KEYLESS VEHICLE REAR PASSENGER DOOR EXTERNAL AERIAL A SIGNAL
16 | 0.35 | 26AL | KEYLESS VEHICLE REAR PASSENGER DOOR EXTERNAL AERIAL B SIGNAL