118

| DASHBOARD WIRING
DG

#### 118
ANTI-LOCK BRAKING SYSTEM COMPUTER
EBASE/SABLAT CA,CAREG/SSESP

1 | 4.0 | MAH | ANTI-LOCK BRAKING SYSTEM ELECTRICAL EARTH
2 | 4.0 | BP8 | PROTECTED + BATTERY FEED > ANTI-LOCK BRAKING SYSTEM MOTOR
3 | 2.5 | BP14 | PROTECTED + BATTERY FEED > ABS
4 | 2.5 | MAH | ANTI-LOCK BRAKING SYSTEM ELECTRICAL EARTH
5 | 0.5 | 4C | LEFT HAND FRONT WHEEL SENSOR SIGNAL
6 | 0.5 | 4H | LEFT HAND REAR WHEEL SENSOR +
8 | 0.5 | 4T | RIGHT HAND REAR WHEEL SENSOR +
9 | 0.5 | 4N | RIGHT HAND FRONT WHEEL SENSOR +
10 | 0.5 | 4M | RIGHT HAND FRONT WHEEL SENSOR SIGNAL
11 | 0.75 | HK | DIAGNOSTIC SIGNAL K
15 | 0.5 | 4DN | ANTI-LOCK BRAKING SYSTEM LOWER CAN SIGNAL
16 | 0.5 | 4E | LEFT HAND FRONT WHEEL SENSOR +
17 | 0.5 | 4G | LEFT HAND REAR WHEEL SENSOR SIGNAL
18 | 0.75 | SP15 | PROTECTED + ACCESSORIES FEED FUSE
19 | 0.5 | 4S | RIGHT HAND REAR WHEEL SENSOR SIGNAL
20 | 0.75 | 65A | BRAKE LIGHTS + CONTROL
23 | 0.75 | 47F | VEHICLE SPEED SIGNAL
26 | 0.5 | 4DM | ANTI-LOCK BRAKING SYSTEM UPPER CAN SIGNAL