997

| ENGINE WIRING
K4J730,K4M764

#### 997
LPG COMPUTER
K4M764/EQGPL

A1 | 0.5 | 3MT | ENGINE CAN L SIGNAL
B1 | 0.5 | 3RD | LIQUEFIED PETROLEUM GAS GAUGE SENDER SIGNAL
C1 | 0.5 | 3RC | LIQUEFIED PETROLEUM GAS ON/OFF SIGNAL
F1 | 0.5 | H7 | REV COUNTER > TOP DEAD CENTRE > COIL > COMPUTER ALTERNATOR SIGNAL
G1 | 1.4 | N | ELECTRONIC EARTH
H1 | 1.4 | N | ELECTRONIC EARTH
A2 | 0.5 | 3MS | ENGINE CAN H SIGNAL
C2 | 0.5 | AP31 | PROTECTED + AFTER IGNITION LPG COMPUTER FUSE
G2 | 1.0 | 3HQ | LPG PRESSURE RELIEF SOLENOID VALVE + CONTROL > COMPUTER
H2 | 1.0 | 3QZ | LIQUEFIED PETROLEUM GAS INJECTOR 3
A3 | 0.5 | 3NU | LIQUEFIED PETROLEUM GAS PRESSURE SENSOR +
B3 | 0.5 | 3NW | LIQUEFIED PETROLEUM GAS PRESSURE SENSOR -
D3 | 0.5 | 3XC | - NATURAL GAS PRESSURE SENSOR URBAN DRIVING
E3 | 0.5 | 3VK | LPG TANK SOLENOID VALVE CONTROL
F3 | 0.5 | 3RB | LIQUEFIED PETROLEUM GAS ACTUATOR CONTROL RELAY
G3 | 1.0 | 3QX | LIQUEFIED PETROLEUM GAS INJECTOR 1 - CONTROL
H3 | 1.0 | 3RA | LIQUEFIED PETROLEUM GAS INJECTOR 4 - CONTROL
A4 | 0.5 | 3YB | LIQUID PETROLEUM GAS GAUGE 5 V SIGNAL
B4 | 0.5 | HK | DIAGNOSTIC SIGNAL K
C4 | 0.5 | 3NV | LIQUEFIED PETROLEUM GAS PRESSURE SENSOR SIGNAL
E4 | 0.5 | 3WP | LPG TANK SOLENOID VALVE RELAY CONTROL
F4 | 0.5 | 3HF | LIQUEFIED PETROLEUM GAS ECU SOLENOID VALVE RELAY - CONTROL
G4 | 1.0 | 3QY | LIQUEFIED PETROLEUM GAS INJECTOR 2 - CONTROL
H4 | 1.4 | 3JZ | LIQUEFIED PETROLEUM GAS INJECTOR + CONTROL