R372

| CONNECTION
ANY TYPE

#### R372
REAR / FASCIA BAND CONNECTION
X84 B84,S84/DG/SPRGAZ/EBASE X84 B84,S84/DG/EQGPL/EBASE

3 | 0.5 | MZ | REAR END PANEL ELECTRICAL EARTH
4 | 0.5 | LPD | PROTECTED RIGHT HAND SIDE LIGHT +
5 | 0.5 | 20G | TAILGATE MOTOR OPEN CONTROL
6 | 0.5 | 20G | TAILGATE MOTOR OPEN CONTROL
1 | 0.35 | 26AM | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL A SIGNAL
2 | 0.35 | 26AN | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL SIGNAL2