1337

| ENGINE WIRING
F4R770,F4R771

#### 1337
SWITCHING PROTECTION UNIT
BVA4/TLMEXI BVM6 BVA4/SSTLMEXI

1 | 1.0 | BP42 | PROTECTED + BATTERY FEED > AUTOMATIC TRANSMISSION COMPUTER
2 | 0.5 | 49Q | - FAN HIGH SPEED CONTROL RELAY
3 | 1.0 | BP31 | PROTECTED + BATTERY FEED INJECTOR FUSE > FUEL PUMP
5 | 1.0 | 38R | AIR CONDITIONING CLUTCH + CONTROL
6 | 0.5 | AP11 | PROTECTED + AFTER IGNITION REVERSING LIGHTS FUSE
6 | 0.5 | AP11 | PROTECTED + AFTER IGNITION REVERSING LIGHTS FUSE
8 | 2.0 | 3BS | IGNITION COIL CONTROL
9 | 0.5 | H66P | REVERSING LIGHTS + CONTROL
10 | 2.0 | AP4 | PROTECTED + AFTER IGNITION AUTOMATIC TRANSMISSION FUSE