1511

| DRIVER'S DOOR WIRING
X84

#### 1511
DRIVER'S REAR TWIN ELECTRIC WINDOWS CONTROL
DD/CPE

2 | 0.35 | 23G | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 1
3 | 0.35 | 23B | ELECTRIC WINDOW DOWN CONTROL > RIGHT HAND REAR QUARTER LIGHT OPEN
4 | 0.35 | MAN | DASHBOARD RIGHT-HAND CROSS MEMBER ELECTRICAL EARTH
5 | 0.35 | 23D | ELECTRIC WINDOW DOWN CONTROL > LEFT HAND REAR QUARTER LIGHT OPEN
6 | 0.35 | 23K | LEFT HAND REAR ELECTRIC WINDOW CONTROL 2