133

| FRONT PASSENGER DOOR WIRING
X84

#### 133
PASSENGER'S SIDE ELECTRIC WINDOW CONTROL
B84,S84/DD/CPE

A1 | 0.35 | 22B | PASSENGER'S ELECTRIC WINDOW DOWN CONTROL
B1 | 0.35 | 22D | FRONT ELECTRIC WINDOW CONTROL 2
A2 | 0.35 | 22A | PASSENGER'S ELECTRIC WINDOW UP CONTROL
B2 | 0.35 | MAM | DASHBOARD LEFT-HAND CROSS MEMBER ELECTRICAL EARTH
A3 | 0.35 | 22C | FRONT ELECTRIC WINDOW CONTROL 1
B3 | 0.5 | LPG | PROTECTED LEFT HAND SIDE LIGHT +