261

| RADIO/MULTIMEDIA DISPLAY INTERMEDIATE WIRING
DD

#### 261
RADIO
NINAV1

6 | 0.35 | 133B | INSTRUMENT PANEL CAN H SIGNAL > COMPUTER
7 | 0.35 | 34DZ | MULTIMEDIA 1 CAN H SIGNAL
8 | 0.22 | 34BR | RADIO CAN H SHUNT SIGNAL
9 | 0.22 | 34BR | RADIO CAN H SHUNT SIGNAL
12 | 0.35 | 34GD | COMMUNICATION START/STOP SIGNAL 1
15 | 0.35 | 133C | INSTRUMENT PANEL CAN L SIGNAL > COMPUTER
16 | 0.35 | 34GA | MULTIMEDIA 1 CAN L SIGNAL
17 | 0.22 | 34BS | RADIO CHANNEL SHUNT SIGNAL
18 | 0.22 | 34BS | RADIO CHANNEL SHUNT SIGNAL